name = Stinger Servo Piston
preview = stingerservopiston_preview.bmp
dir = s1_stingerservopiston
model = stingerservopiston4.gmf
type = mechanics
base = ServoPiston
master = body
passthru = shaft_collision
attaching = shaft
prismatic = body, shaft, 0, 0, 1, 0.0, -1.0, 0.2
description = The stinger servo piston allows slow, controlled movement in both in and out directions and has a compression enhancer for 2 times the power. Multiple lengths are available. Wire a button or analog control to this unit.
power = 1 40
airmaxinoutrate = -100
attachsound = sounds\cmp_generic.wav
standard = 1