name = Rooster Servo
preview = chicken_preview.bmp
dir = chicken
model = chicken.gmf
type = mechanics
base = ServoMotor
master = motor
passthru = axle, motor
attaching = axle
description = A micro sized powerful servo.
attachsound = sounds\chickens.wav
standard = 0
power = 3 48000
hitpoints = 3000
motorsound = Sounds\motorloop2.wav
elecmaxinoutrate = -10
alwaysvisible = true