name = Electric Catch-Spring Burst
preview = cs_preview.bmp
dir = snapper2
model = snapper2.gmf
type = mechanics
base = BurstMotor
master = bmotor_body
passthru = axle_collision
styles = Default
description = A burst released when a caught spring is released, producing 125 psi. 
elecMaxInOutRate = -60
burst = 0 50 140
power = 5 120
sort = 11
mass = 8
firesound = sounds\longpneumatic2.wav
attachsound = sounds\cmp_generic.wav
standard = 1