name = DSL Servo Motor 
dir = dslservo
type = mechanics
base = ServoMotor
model = dslservomotor2.gmf
description = Low powered servo motor, useful for slow, controlled rotation of attached objects.  It draws 5.6 amps.
passthru = axle_collision
master = motor
attaching = axle
power = 6 1005
elecMaxInOutRate = -56
runsequence = Sounds\motor_spinup.wav, Sounds\motorloop.wav,Sounds\motor_spindown.wav
attachsound = sounds\cmp_generic.wav
standard = 1