name = Perm motors
preview = perm_preview.bmp
dir = perm
model = perm80_L.gmf
type = mechanics
base = SpinMotor
master = motor
passthru = axle_collision
attaching = axle
description = This is the Perm 80 with 4-1 gearing.  Exactly like the normal Perm 80, but "only" 1720 rpm and four times the torque.  This version has the long belt.
elecMaxInOutRate = -38000
power = 172 36
sort = 1
motorsound = sounds\motorloop.wav
attachsound = sounds\cmp_generic.wav
standard = 1
alwaysvisible = true
mass=30