name = VDMA Servo Piston
preview = pistons_preview.bmp
dir = pistons
model = vdmamed2.gmf
type = mechanics
base = ServoPiston
master = body
passthru = shaft_collision
attaching = shaft
prismatic = body, shaft, 0, 0, 1, 0.0, -0.50, .8
description = The servo piston moves forward and back in a controlled manner.  Wire with an analog control.
airmaxinoutrate = -18
power = 40 40
force = 1000000
sort = 30
firesound = sounds\air_trigger.wav
attachsound = sounds\cmp_airtank.wav
standard = 1
mass = 28