name = DSL linear actuator
preview = servopiston_preview.bmp
dir = pistons
model = vdmaservo3.gmf
type = mechanics
base = ServoPiston
master = body
passthru = shaft_collision
attaching = shaft
prismatic = body, shaft, 0, 0, 1, 0.0, -0.37, .8
styles = 80 cm, servopiston2.txt, 100 cm, servopiston3.txt, 120 cm
description = DSL linear actuator fires its shaft at a high velocity In both directions. 
airmaxinoutrate = -100
power = 900 40
sort = 30
firesound = sounds\air_trigger.wav
attachsound = sounds\cmp_airtank.wav
mass = 30
standard = 1